**J23-63T Electric Power Press**

**Features:**

* With an inclinable cast structure, the machine body can incline to allow a punched work-piece or waste material to slide down from the die.
* With a rigid turn-key clutch, the press has single or continuous operation standards.
* The punch press uses a single type brake. The sliding block is equipped with a press-down type safety device that can be pressed down to protect the entire machine.
* Avoid being damaged in case of overpressure.
* The machine has the advantages of high universality, high precision, reliable performance and convenient operation.

|  |  |  |  |
| --- | --- | --- | --- |
| No. | Item. | Unit | J23-63T |
| 1 | Nominal Force | KN | 630 |
| 2 | Throat Depth | mm | 280 |
| 3 | Slide Stroke | mm | 100 |
| 4 | Slipper Stroke Times | times/min | 50 |
| 5 | Shut Height | mm | 380 |
| 6 | Shut Height Adjustable | mm | 60 |
| 7 | Angle of Inclination | degree | 20 |
| 8 | Column Distance | mm | 350 |
| 9 | Table Size | mm | 450×700 |
| 10 | Table Thickness | mm | 80 |
| 11 | Motor Power | KW | 4.0 |
| 12 | Slide bottom size | Front and Back  | 220mm |
|  | Left and Right | 310mm |
| 13 | Weight | kg | 3100 |
| 14 | Dimension | mm | 1500×1200×2400 |