**J23-63T Electric Power Press**

**Features:**

* With an inclinable cast structure, the machine body can incline to allow a punched work-piece or waste material to slide down from the die.
* With a rigid turn-key clutch, the press has single or continuous operation standards.
* The punch press uses a single type brake. The sliding block is equipped with a press-down type safety device that can be pressed down to protect the entire machine.
* Avoid being damaged in case of overpressure.
* The machine has the advantages of high universality, high precision, reliable performance and convenient operation.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Item. | | Unit | | J23-63T |
| 1 | Nominal Force | | KN | | 630 |
| 2 | Throat Depth | | mm | | 280 |
| 3 | Slide Stroke | | mm | | 100 |
| 4 | Slipper Stroke Times | | times/min | | 50 |
| 5 | Shut Height | | mm | | 380 |
| 6 | Shut Height Adjustable | | mm | | 60 |
| 7 | Angle of Inclination | | degree | | 20 |
| 8 | Column Distance | | mm | | 350 |
| 9 | Table Size | | mm | | 450×700 |
| 10 | Table Thickness | | mm | | 80 |
| 11 | Motor Power | | KW | | 4.0 |
| 12 | Slide bottom size | Front and Back | | 220mm | |
|  | | Left and Right | | 310mm | |
| 13 | Weight | | kg | | 3100 |
| 14 | Dimension | | mm | | 1500×1200×2400 |