Fixed Carbon                      80 - 85%,

Ash                                        4%

Electrical Resistance        80 micro ohm/m

Volatility                             12 -14%

Apparent Density  (Fluidity coefficient)      1,6 - 2,8%